{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1 (2)","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1 (2)","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["广东茂名农林科技职业学院\n网络信息中心服务队维护设备及耗材采购清单"]
["序号","工具名称","参数","数量","单位","单价（元）","总价（元）"]
[1,"工具存放柜","850*390*1800  1.基材：采用国标优质0.5MM厚冷轧钢板经剪切、冲压、折弯、焊接、装配而成，喷塑前均经磷化处理；2.柜面：柜面采用绿色环保型粉沫，高温塑化而成，防腐性好，环保耐用，色彩柔和，光洁美，使用时无异味。。",1,"个"]
[2,"电动手枪钻","电动工具：扭矩最大扭矩(硬扭/软扭) 28/11牛顿米\n空载速率：齿轮1 0-400转/分钟 齿轮2 0-1500转/分钟\n最大钻孔直径： 钢材 6毫米 木材 19毫米 砖墙 8毫米\n电钻/冲击钻/锂电手电钻\n包装清单 1*裸机 1*充电器 2*电池\"",1,"套"]
[3,"220V电钻","\n220V正反调速多功能电钻  冲击率0-44800次/分钟",1,"台"]
[4,"冲击钻","额定电压(V)220\n额定功率(W)600\n木材金属混凝土等材质钻孔\n带卡钻离合器\n木材金属混凝土等材质钻孔",1,"台"]
[5,"电烙铁","功率60W 输入电压 220V 50hz 温度 600°C 加热方式 外热式 发热元件 重绕式 镍铬丝发热芯",3,"套"]
[6,"铝梯","产品净重（kg）5\n产品承重（kg）150\n使用尺寸（cm）190\n收纳尺寸（cm）200\n包装尺寸（cm）200",2,"把"]
[7,"钻头","十字",2,"盒"]
[8,"模块打线刀","冲击力强 双刀头设计",2,"把"]
[9,"套铜","11件套",1,"套"]
[10,"安全带","欧式涤沦缓冲双大钩",2,"套"]
[11,"吸吹风机","一电一充带收纳箱",1,"台"]
[12,"水口钳","斜口斜嘴水口钳工业级",3,"把"]
[13,"老虎钳","钢丝钳，镍铬合金钢",3,"把"]
[14,"线槽剪","8寸多功能电工剪\n剥线 剪线 剪铁皮 压接",3,"把"]
[15,"螺丝刀套装","镍铬合金钢 螺丝刀",5,"套"]
[16,"笔记本维修螺丝刀套装","螺丝批60只，包装盒一个",3,"套"]
[17,"焊锡丝","焊锡丝",2,"圈"]
[18,"网络钳","具有剪、压、剥线功能\n功能用途\n4P/6P/8P网络压接钳",3,"把"]
[19,"测线器","\n\n可测网线，电话线的通断、交叉、短路、断路等多种线路状态\n",3,"把"]
[20,"寻线器","具有寻线、对线、线路状态测试三大功能",3,"套"]
[21,"光纤笔","功率测量范围dBm -70^+10 -50~+26\n波长测量范围 800^1700\n校准波长nm 850、 980、 1300、 1310、 1490、 1550、 1625\n探头类型 InGaAs\n测量精度 <±3%(-10dBm 20 *C)\n显示分辨率dB 线性显示：0.1%,对数显示：0.01 dBm\n工作温度C 0 -10~+50\n储存温度C -20~+70\n相对湿度 90% (+30-C),不凝结\n光接口 SC/FC (STLC 选购)\n电池连续工作时间 120小时（仅光功）\n电源 2000ma锂电池\n自动关机时间min 10 J\n重量g 270\n外形尺寸mm 166*84*34\n红光（功能选件） 波长650nm,功率 1~30mw. OHz^ 2Hz  ",1,"支"]
[22,"数显测电笔","产品名称 数显测电笔  产品品牌 征伏\n电笔头部 一字型\n产品特点 多功能测电笔 产品材质 铭机合金钢，ABS\n使用范围 适用于直接检测12-250V的交、直流电和间接检测交流电的零钱、相线和断点， 还可检测不带电导体的通断",3,"套"]
[23,"万用表","主机，表笔，电池，说明书，合格证。",3,"个"]
[24,"电流表","直流电压  600V ±1.0%+6d 分济力 1V\n交流电压  600V ±1.0%+10d 分辨力 1V\n交流电流  2/20/200/600A ±2.5%+8d 0.1A\n电阻测量  2000 Q/200K Qt 1.0%+5d 0.1 Q 忌体\n电容测量  200pF ±(4.0%+10)分辨力lOOnf\n二极管测量  开路约1.4V正向压降0.5~0.8V分辨力1mV\n通断蜂鸣  开路电压约0.45V低于50-70Q发声\n测量方式 双积分式A/D转换\n转换速率 3次渺\n超量程显示 高位显示\n低电压提示 缺电符号显示\n",3,"个"]
[25,"内六角套装","内六角扳手套装",3,"套"]
[26,"梅花套装","\n9件套(1.5-10MM)扳手组套\n",3,"套"]
[27,"主板测试卡","\n笔记本台式机诊断卡\n",3,"套"]
[28,"工具包","材质 牛津布\n名称 多功能工具包 长度 400mm\n宽度 220mm 重量 1025g",3,"个"]
[29,"网线"," 6类4对非屏蔽双绞线（低烟无卤）\n单位 305米/箱",610,"米"]
[30,"水晶头","\n水晶头RJ15高速 耐用",5,"盒"]
[31,"U盘","128GB USB3.0 U盘",5,"个"]
[32,"讲台电子屏","面板类型TN\n最佳分辨率1920×1080\n点距0.248mm\n对比度动态对比度：10,000,000：1\n色数16.7M\n刷新率60Hz\n亮度200cd/m2\n可视角度90º (H) / 65º (V) @ C/R > 10\n屏幕比例16:9\n响应时间5ms\n面板尺寸21.5英寸\n",2,"台"]
[33,"键盘鼠标","键盘规格\n接口USB\n键盘标准89-108键\n重量（g）550g\n尺寸（mm）450x155x23.5mm\n包装清单键盘x1;鼠标x1;用户文档x1",6,"套"]
[34,"面板","86型国标",10,"个"]
[35,"电动投影幕电机","200寸（4：3）",1,"个"]
[36,"电动投影幕电机","180寸（4：3）",1,"个"]
[37,"电动投影幕电机","150寸（4：3）",2,"个"]
[38,"鹅颈话筒","换能方式:电容式\n指向特性:超心型指向\n频率响应:70-20KHZ 灵敏度：-45dB(±2dB)\n输出阻抗：200Q 电源供应:DC3/AC220V\n其他特点:可抗珈干扰，电磁干扰",6,"套"]
[39,"维修工作桌椅","台：1200*600*750采用环保三聚氰胺板，具有防潮，不发霉等特点，进口PVC胶边封边。  \n椅子：440*430*930采用实木框架，贴木皮凳面，榫卯结构，经防潮,防腐,防虫化学处理，经过干燥处理使之不易变形",6,"套"]
[40,"合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}